{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Fan","Air flow rate","Cooling","Super low","m³/min","30","","","34"]
["","","Heating","Super low","m³/min","32","","","34"]
["Sound power level","Heating","","","dBA","","","62","","62"]
["","Cooling","","","dBA","","","60","","60"]
["Fan","Air flow rate","Cooling","Super low","cfm","1059","","","1200"]
["","","Heating","Super low","cfm","1130","","","1200"]
["Dimensions","Unit","","Height","mm","550","550","550","550","550","550"]
["","","","Width","mm","765","765","765","765","765","765"]
["","","","Depth","mm","285","285","285","285","285","285"]
["Weight","Unit","","","kg","36","36","36","41","41","41"]
["Fan motor","Speed","Cooling","Super low","rpm","760","500","500","890","500","500"]
["","","Heating","Super low","rpm","820","320","320","890","500","500"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","","46.0","-10","46.0"]
["","","","Max.","°CDB","46","","-10","46","-10"]
["","Heating","Ambient","Min.","°CWB","-15","","-15","-15","-15.0"]
["","","","Max.","°CWB","18","","18.0","18","18.0"]
["Sound pressure level","Cooling","","High","dBA","","46","46","","48","48"]
["","","","Nom.","dBA","48","","","46"]
["","Heating","","High","dBA","","48","48","","50","50"]
["","","","Nom.","dBA","50","","","48"]
["Refrigerant","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Charge","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","GWP","","","","675","675.0","675","675","675","675"]
["Piping connections","Piping length","OU - IU","Max.","m","20","20","20 (1)","20","20 (1)","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","m","15","15.0","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Total piping length","System","Actual","m","30","30","30","30","30","30"]
["Standard Accessories","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Notes","","","","","","(1) - For one room","","","","(1) - For one room"]
["","","","","","","","(1) - For one room","","(1) - For one room"]
["","","","","","","","(2) - See separate drawing for operation range","","(2) - See separate drawing for operation range"]
["","","","","","","","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data"]
["","","","","","","","(4) - Contains fluorinated greenhouse gases","","(4) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Reducer assembly","","","","","","","1","1","1"]