{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":9,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Screw+Washer","","","","Screw+Washer","Screw+Washer"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","Cover lock grill"]
["","Battery","","","","Battery","Battery"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.88"]
["","Drain","","","","19.05"]
["Power input","Cooling","","Nom.","kW","0.128"]
["","Heating","","Nom.","kW","0.128"]
["Sound power level","Cooling","","","dBA","64"]
["","Heating","","","dBA","64"]
["Dimensions","Unit","","Width","mm","600"]
["","","","Depth","mm","1,007"]
["","","","Height","mm","285"]
["Casing","Material","","","","Galvanised steel"]
["Weight","Unit","","","kg","35"]
["Fan","External static pressure","","High","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Low","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Name","","","","V1"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Power input","Heating","","Nom.","kW","","0.109"]
["","Cooling","","Nom.","kW","","0.109"]
["Fan","External static pressure","","High","Pa","","70","150","150"]
["","","","Low","Pa","","45","111","92"]
["Casing","Material","","","","","Galvanised steel"]
["Dimensions","Unit","","Height","mm","","378","378","378"]
["","","","Width","mm","","541","1300","1500"]
["","","","Depth","mm","","1045","541","541"]
["Weight","Unit","","","kg","","44","50","56"]
["Fan","Air flow rate","Cooling","High","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Low","m³/min","","18.3","34.8","37.9"]
["","","Heating","High","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Low","m³/min","","18.3","34.8","37.9"]
["","External static pressure","","Nom.","Pa","","57","128","122"]
["Sound power level","Cooling","","","dBA","","60","72","73"]
["","Heating","","","dBA","","60","72","73"]
["Sound pressure level","Cooling","","High","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Low","dBA","","36","50","50"]
["","Heating","","High","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Low","dBA","","36","50","50"]
["Piping connections","Liquid","","OD","mm","","9.52","9.52","9.52"]
["","Gas","","OD","mm","","15.88","15.9","15.9"]
["","Drain","","","","","19.05"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10","13.00"]
["Heating capacity","Total capacity","","Nom.","kW","","","13.5","15.5"]
["Casing","Colour","","","","","","Galvanised steel plate / Not painted","Galvanised steel plate / Not painted"]
["Fan","Air flow rate","Cooling","Medium","m³/min","","","37","44"]
["","","Heating","Medium","m³/min","","","37.4","43.9"]
["Sound pressure level","Cooling","","Medium","dBA","","","52","53"]
["","Heating","","Medium","dBA","","","52","53"]
["Control systems","Infrared remote control","","","","","","ARCWLA","ARCWLA"]