{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L"]
[]
[]
[]
[]
["","","","","ADEQ50C2VEB / ARXS50L2V1B","ADEQ60C2VEB / ARXS60L2V1B","ADEQ71C2VEB / ARXS71L2V1B"]
["Cooling capacity","Nom.","","kW","5.00 (1)","5.70 (1)","6.80 (1)"]
["Space cooling","SEER","","","5.60","5.70","5.30"]
["","Annual energy consumption","","kWh/a","313","350","449"]
["","Capacity","Pdesign","kW","5.00","5.70","6.80"]
["","Energy efficiency class","","","A+","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.40","4.60","6.00"]
["","SCOP/A","","","4.00","4.00","3.80"]
["","Energy efficiency class","","","A+","A+","A"]
["","Pdh Heating capacity at -10°","","kW","3.69","3.91","4.83"]
["","Annual energy consumption","","kWh/a","1,540","1,610","2,210"]
["Heating capacity","Nom.","","kW","5.50 (1)","7.00 (1)","7.50 (1)"]
["Notes","","","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(2) - EER/COP according to Eurovent 2012, for use outside EU only","(2) - EER/COP according to Eurovent 2012, for use outside EU only","(2) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2"]
["","","","","(5) - See separate drawing for electrical data","(5) - See separate drawing for electrical data","(5) - See separate drawing for electrical data"]
["","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]