{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Cooling capacity","Nom.","","kW","3.40 (1)"]
["Space cooling","SEER","","","5.70"]
["","Annual energy consumption","","kWh/a","209"]
["","Capacity","Pdesign","kW","3.40"]
["","Energy efficiency class","","","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.90"]
["","SCOP/A","","","4.00"]
["","Energy efficiency class","","","A+"]
["","Pdh Heating capacity at -10°","","kW","2.47"]
["","Annual energy consumption","","kWh/a","1,015"]
["Heating capacity","Nom.","","kW","4.00 (1)"]
["Notes","","","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(2) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2"]
["","","","","(5) - See separate drawing for electrical data"]
["","","","","(6) - Contains fluorinated greenhouse gases"]