{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ALD-HEFB"]
[]
[]
[]
[]
["","","","","ALD02HEFBU00","ALD03HEFBU00","ALD05HEFBU00","ALD07HEFBU00"]
["Connectable unit","","","","ALB02LB, ALB02RB","ALB03LB, ALB03RB","ALB05LB, ALB05RB, ALB04LB, ALB04RB","ALB06LB, ALB06RB, ALB07LB, ALB07RB"]
["LED indicators","","","","Airflow fault - Yellow, Heat ON - Red","Airflow fault - Yellow, Heat ON - Red","Airflow fault - Yellow, Heat ON - Red","Airflow fault - Yellow, Heat ON - Red"]
["Capacity","kW","","","1.5","3.0","7.5","15.0"]
["Mounting holes","","","","Depends on duct size","Depends on duct size","Depends on duct size","Depends on duct size"]
["Maximum ambient adjacent to terminal box","","","","30°C (during operation)","30°C (during operation)","30°C (during operation)","30°C (during operation)"]
["Dimensions","Unit","Width","mm","470","620","720","920"]
["","","Depth","mm","370","370","370","370"]
["","","Height","mm","193","243","343","443"]
["Temperature sensor","","","","10 kΩ at +20°C, 15 kΩ at -20°C","10 kΩ at +20°C, 16 kΩ at -20°C","10 kΩ at +20°C, 17 kΩ at -20°C","10 kΩ at +20°C, 18 kΩ at -20°C"]
["Temperature control range","","","","-20…10°C","-20…10°C","-20…10°C","-20…10°C"]
["Control fuse","","","","Mini Circuit Breaker 6 A","Mini Circuit Breaker 6 A","Mini Circuit Breaker 6 A","Mini Circuit Breaker 6 A"]
["Power supply","Phase","","","1~","1~","3~","3~"]
["","Voltage","","V","230","230","400","400"]