{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Sound pressure level","Heating","","High","dBA","","48"]
["","","","Low","dBA","","45"]
["Standard Accessories","1","","","","","550"]
["Refrigerant","Charge","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Fan","Air flow rate","Cooling","Super low","m³/min","","30.1"]
["","","","Super low","cfm","","1,063"]
["Fan motor","Speed","Cooling","Super low","rpm","","740"]
["","","Heating","Super low","rpm","","-15"]
["Operation range","Heating","Ambient","Min.","°CWB","","20"]
["","","","Max.","°CWB","","10"]
["Sound pressure level","Cooling","","Low","dBA","","44"]
["","","","High","dBA","","48"]
["Dimensions","Unit","","Width","mm","","285"]
["","","","Depth","mm","","612"]
["","","","Height","mm","","765"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","34"]
["Fan","Air flow rate","Heating","Super low","cfm","","904"]
["","","","Super low","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","(1) - 220V","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Fan","Air flow rate","Cooling","Super low","m³/min","30.1"]
["","","Heating","Super low","m³/min","25.6"]
["","","","Super low","cfm","1063"]
["","","Heating","Super low","cfm","904"]
["Dimensions","Unit","","Height","mm","550"]
["","","","Width","mm","765"]
["","","","Depth","mm","285"]
["Weight","Unit","","","kg","34"]
["Fan motor","Speed","Cooling","Super low","rpm","780"]
["","","Heating","Super low","rpm","740"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Heating","Ambient","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Sound pressure level","Cooling","","High","dBA","46"]
["","Heating","","High","dBA","47"]
["","","","Low","dBA","44"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","1.0"]
["","Charge","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]