{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTM-A"]
[]
[]
[]
[]
["","","","","","ATXTM30A2V1B"]
["Power input","Cooling","","Nom.","kW","0.029"]
["","Heating","","Nom.","kW","0.024"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","298"]
["","","","Width","mm","804"]
["","","","Depth","mm","252"]
["Weight","Unit","","","kg","12"]
["Fan","Air flow rate","Cooling","High","m³/min","13.2"]
["","","","Medium","m³/min","8.1"]
["","","","Low","m³/min","5.6"]
["","","","Silent operation","m³/min","4.8"]
["","","Heating","High","m³/min","11.7"]
["","","","Medium","m³/min","7.7"]
["","","","Low","m³/min","5.6"]
["","","","Silent operation","m³/min","4.7"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","59"]
["Sound pressure level","Cooling","","High","dBA","45"]
["","","","Medium","dBA","33"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","21"]
["","Heating","","High","dBA","43"]
["","","","Medium","dBA","31"]
["","","","Low","dBA","22"]
["","","","Silent operation","dBA","19"]
["Refrigerant","GWP","","","","675"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.5"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A83"]
["Standard Accessories","ATXTM30A2V1B","","","","1"]
["","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - See separate drawing for electrical data"]