{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53C"]
[]
[]
[]
[]
["","","","","BRC1E53C7"]
["Packing","Material","","","Carton"]
["","Weight","","kg","0.05"]
["Ambient temperature","Relative humidity <","","%","95"]
["Dimensions","Packed unit","Width","mm","160"]
["","","Height","mm","55"]
["","","Depth","mm","150"]
["","Unit","Width","mm","120"]
["","","Depth","mm","19"]
["","","Height","mm","120"]
["Casing","Button cover","","","No"]
["","Colour","","","Fresh White"]
["","Operation LED","Colour","","Green"]
["LCD","Type","","","Full dot (160 x 255)"]
["","Back light","Colour","","White"]
["","Dimensions","Width","mm","68.85"]
["","","Height","mm","43.2"]
["Weight","Packed unit","","kg","0.415"]
["","Unit","","kg","0.200"]
["Wiring connections","Wiring length","Max.","m","500"]
["Back-up for power failure","","","","Yes (The clock will keep functioning for a period not exceeding 48 hours)"]