{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":17,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVH-D9W7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EAVH16S18DA9W7 / EPGA11DAV37","EAVH16S18DJ9W7 / EPGA11DAV37","EAVH16S23DA9W7 / EPGA11DAV37","EAVH16S23DJ9W7 / EPGA11DAV37","EAVH16S18DA9W7 / EPGA14DAV37","EAVH16S18DJ9W7 / EPGA14DAV37","EAVH16S23DA9W7 / EPGA14DAV37","EAVH16S23DJ9W7 / EPGA14DAV37","EAVH16S18DA9W7 / EPGA16DAV37","EAVH16S18DJ9W7 / EPGA16DAV37","EAVH16S23DA9W7 / EPGA16DAV37","EAVH16S23DJ9W7 / EPGA16DAV37"]
["Domestic hot water heating","General","","Declared load profile","","L","L","XL","XL","L","L","XL","XL","L","L","XL","XL"]
["","Average climate","","Water heating energy efficiency class","","A","A","A","A","A","A","A","A","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Indoor unit","","","","","EAVH16S18DA9W7","EAVH16S18DJ9W7","EAVH16S23DA9W7","EAVH16S23DJ9W7","EAVH16S18DA9W7","EAVH16S18DJ9W7","EAVH16S23DA9W7","EAVH16S23DJ9W7","EAVH16S18DA9W7","EAVH16S18DJ9W7","EAVH16S23DA9W7","EAVH16S23DJ9W7"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","172","172","172","172","175","175","175","175","179","179","179","179"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","","","SCOP","","4.38","4.38","4.38","4.38","4.45","4.45","4.45","4.45","4.56","4.56","4.56","4.56"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","129","129","129","129","130","130","130","130","133","133","133","133"]
["","","","SCOP","","3.29","3.29","3.29","3.29","3.34","3.34","3.34","3.34","3.41","3.41","3.41","3.41"]
["Heat up time from 10°C to 50°C","hr","","","","53min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature"]
["Heating capacity","Nom.","","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Power input","Heating","","Nom.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.67","2.67","3.08","3.08","2.67","2.67","3.08","3.08","2.67","2.67","3.08","3.08"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]