{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBBH-D6V / ERLA11-14DV3"]
[]
[]
[]
[]
["","","","","","EBBH11DF6V / ERLA11DAV3","EBBH11DF6V / ERLA11D2V3","EBBH16DF6V / ERLA14DAV3","EBBH16DF6V / ERLA14D2V3"]
["Heating capacity","Nom.","","","kW","10.6 (1), 9.82 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)","12.0 (1), 12.5 (2)"]
["Power input","Heating","","Nom.","kW","2.18 (1), 2.68 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.83 (1), 3.66 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)","4.87 (1), 3.64 (2)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.23","3.23","3.22","3.22"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.63","4.63","4.60","4.60"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(4) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(4) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(4) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°.","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°.","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°.","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°."]
["Energy Efficiency Range","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]