{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA-DV37"]
[]
[]
[]
[]
["","","","","","EBLA16DAV37"]
["Heating capacity","Nom.","","","kW","16.0 (2) (1)"]
["Cooling capacity","Nom.","","","kW","14.0 (3), 15.3 (4)"]
["Power input","Cooling","","Nom.","kW","4.58 (3), 3.24 (4)"]
["","Heating","","Nom.","kW","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)"]
["EER","","","","","3.06 (3), 4.74 (4)"]
["Dimensions","Unit","","Height","mm","870"]
["","","","Width","mm","1380"]
["","","","Depth","mm","460"]
["Weight","Unit","","","kg","147"]
["Fan","Air flow rate","Heating","High","m³/min","85.0"]
["","","Cooling","High","m³/min","85.0"]
["Operation range","Heating","Water side","Min.","°C","9 (6)"]
["","","","Max.","°C","60 (6)"]
["","Cooling","Ambient","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","","Water side","Min.","°C","5"]
["","","","Max.","°C","22"]
["","Domestic hot water","Ambient","Min.","°CDB","-25"]
["","","","Max.","°CDB","35"]
["","","Water side","Min.","°C","25"]
["","","","Max.","°C","55 (6)"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675"]
["","Charge","","","kg","3.80"]
["","Charge","","","tCO2Eq","2.57"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.37"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.69"]
["","","","Seasonal space heating eff. class","","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Compressor component","Main power supply","","Phase","","1~"]
["","","","Voltage","V","230"]
["Power supply","Name","","","","V3"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(5) - According to EN14825"]
["","","","","","(6) - For more details, see operation range drawing"]
["","","","","","(7) - Depends on operation mode, refer to installation manual."]