{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA09-14D3V3"]
[]
[]
[]
[]
["","","","","","EBLA09DA3V3","EBLA11DA3V3","EBLA14DA3V3"]
["Heating capacity","Nom.","","","kW","9.37 (1), 9.00 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Cooling capacity","Nom.","","","kW","9.35 (3), 9.10 (4)","11.6 (3), 11.5 (4)","12.8 (3), 12.7 (4)"]
["Heater capacity","Step 1","","","kW","3","3","3"]
["Power input","Cooling","","Nom.","kW","2.79 (3), 1.71 (4)","3.56 (3), 2.17 (4)","4.06 (3), 2.51 (4)"]
["","Heating","","Nom.","kW","1.91 (1), 2.43 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.91 (1), 3.71 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["EER","","","","","3.35 (3), 5.34 (4)","3.26 (3), 5.31 (4)","3.16 (3), 5.04 (4)"]
["Dimensions","Unit","","Height","mm","870","870","870"]
["","","","Width","mm","1380","1380","1380"]
["","","","Depth","mm","460","460","460"]
["Weight","Unit","","","kg","149","149","149"]
["Fan","Air flow rate","Heating","High","m³/min","48.0","55.8","70.4"]
["","","Cooling","High","m³/min","63.1","70.4","85.0"]
["Operation range","Heating","Water side","Min.","°C","15 (6)","15 (6)","15 (6)"]
["","","","Max.","°C","60 (6)","60 (6)","60 (6)"]
["","Cooling","Ambient","Min.","°CDB","10","10","10"]
["","","","Max.","°CDB","43","43","43"]
["","","Water side","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["","Domestic hot water","Ambient","Min.","°CDB","-25","-25","-25"]
["","","","Max.","°CDB","35","35","35"]
["","","Water side","Min.","°C","25","25","25"]
["","","","Max.","°C","55 (6)","55 (6)","55 (6)"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","3.80","3.80","3.80"]
["","Charge","","","tCO2Eq","2.57","2.57","2.57"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.44","3.37","3.42"]
["","","","Seasonal space heating eff. class","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.82","4.73","4.70"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++"]
["Compressor component","Main power supply","","Phase","","1~","1~","1~"]
["","","","Voltage","V","230","230","230"]
["Power supply","Name","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(5) - According to EN14825","(5) - According to EN14825","(5) - According to EN14825"]
["","","","","","(6) - For more details, see operation range drawing","(6) - For more details, see operation range drawing","(6) - For more details, see operation range drawing"]
["","","","","","(7) - Depends on operation mode, refer to installation manual.","(7) - Depends on operation mode, refer to installation manual.","(7) - Depends on operation mode, refer to installation manual."]