{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWETU-BV3"]
[]
[]
[]
[]
["","","","","","EKHWETU120BAV3"]
["Mounting","","","","","Wall"]
["Casing","Colour","","","","White, Black"]
["","Material","","","","Sheet metal, Acrylonitrile Butadiene Styrene"]
["Dimensions","Unit","Height","Tank","mm","1283"]
["","","","Width","mm","510"]
["","","","Depth","mm","570"]
["Weight","Unit","","Empty","kg","47"]
["Tank","Water volume","","","l","118"]
["","Material","","","","Enamel coated steel acc. DIN4753TL2"]
["","Maximum water temperature","","","°C","70"]
["","Energy efficiency class","","","","C"]
["Heat exchanger","Domestic hot water","","Quantity","","1"]
["","","","Tube material","","Aluminium"]
["","","","Operating pressure","bar","42"]
["Booster heater","Capacity","","","kW","1"]
["Energy Efficiency Range","","","","","A+ ~ F"]