{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWSU-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWSU150D3V3","EKHWSU180D3V3","EKHWSU200D3V3","EKHWSU250D3V3","EKHWSU300D3V3"]
["Booster heater","Capacity","","","kW","3","3","3","3","3"]
["Heat exchanger","Domestic hot water","","Tube material","","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)"]
["","","","Operating pressure","bar","10","10","10","10","10"]
["","","","Internal coil volume","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Quantity","","1","1","1","1","1"]
["Dimensions","Unit","","Diameter","mm","595","595","595","595","595"]
["","","Height","Tank","mm","1,000","1,164","1,264","1,535","1,745"]
["Casing","Material","","","","Epoxy coated steel, Epoxy-coated mild steel","Epoxy coated steel, Epoxy-coated mild steel","Epoxy coated steel, Epoxy-coated mild steel","Epoxy coated steel, Epoxy-coated mild steel","Epoxy coated steel, Epoxy-coated mild steel"]
["","Colour","","","","Neutral white","Neutral white","Neutral white","Neutral white","Neutral white"]
["Tank","Energy efficiency class","","","","B","B","B","B","B"]
["","Maximum water temperature","","","°C","75","75","75","75","75"]
["","Material","","","","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)"]
["","Water volume","","","l","145","174","192","242","292"]
["Weight","Unit","","Empty","kg","45","50","53","58","63"]
["","","","Full","kg","190","224","245","300","355"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]