{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMBGU-A"]
[]
[]
[]
[]
["","","","","","EKOMBGU22AAV1","EKOMBGU28AAV1","EKOMBGU33AAV1"]
["Gas","Connection","","Diameter","mm","15","15","15"]
["","Consumption (G20)","","Min","m³/h","0.58","0.74","0.79"]
["","","","Max","m³/h","2.29","2.91","3.39"]
["","Consumption (G31)","","Min","m³/h","0.22","0.28","0.30"]
["","","","Max","m³/h","0.87","1.11","1.29"]
["","NOx class","","","","6","6","6"]
["","NOx level (G20)","","","mg/kWh","38","55","34"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","5.6","7.1","7.6"]
["","","","Max","kW","18.7","23.7","27.0"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","6.2","7.9","8.4"]
["","","","Max","kW","20.8","26.3","30.0"]
["","Output Pn at 80/60°C","","Nom","kW","18.2","23.1","26.6"]
["","Output at 37/30°C","","Nom","kW","6.1","7.7","8.8"]
["","Water temperature","","Max","°C","90","90","90"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","5.6","7.1","7.6"]
["","","","Max","kW","22.1","28.0","32.7"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","6.2","7.9","8.4"]
["","","","Max","kW","24.5","31.1","36.3"]
["","Comfort class (EN13203)","","","","L","XL","XL"]
["","Temperature","","Max","°C","65","65","65"]
["Space heating","General","","ηs (Seasonal space heating efficiency)","%","92","92","93"]
["","","","Seasonal space heating eff. class","","A","A","A"]
["Supply air","Concentric","","","","60/100","60/100","60/100"]
["Flue gas","Temperature","","Max","°C","70","70","70"]
["","Mass flow (G20)","","Max","kg/h","36.7","46.8","54.4"]
["","Mass flow (G31)","","Max","kg/h","36.4","46.1","53.6"]
["Casing","Colour","","","","RAL9010","RAL9010","RAL9010"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","590","650","710"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","XL"]
["","","","Water heating energy efficiency class","","A","A","A"]