{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKVDX-A"]
[]
[]
[]
[]
["","","","","EKVDX32A2VEB","EKVDX50A2VEB","EKVDX80A2VEB","EKVDX100A2VEB"]
["Operation range","Around unit","","°CDB","10°C~40°CDB, 80% RH or less","10°C~40°CDB, 80% RH or less","10°C~40°CDB, 80% RH or less","10°C~40°CDB, 80% RH or less"]
["Weight","Unit","","kg","19.0","23.4","30.1","37.7"]
["Refrigerant","Control","","","Motor operated expansion valve","Motor operated expansion valve","Motor operated expansion valve","Motor operated expansion valve"]
["","GWP","","","675.0, 2,087.5","675.0, 2,087.5","675.0, 2,087.5","675.0, 2,087.5"]
["","Type","","","R32/R410A","R32/R410A","R32/R410A","R32/R410A"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","OD","mm","12.7","12.7","12.7","12.7"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","VP20 (I.D. 20/O.D. 26), drain height 625 mm","VP20 (I.D. 20/O.D. 26), drain height 625 mm","VP20 (I.D. 20/O.D. 26), drain height 625 mm","VP20 (I.D. 20/O.D. 26), drain height 625 mm"]
["Dimensions","Unit","Width","mm","550","700","1,000","1,400"]
["","","Depth","mm","809","809","809","809"]
["","","Height","mm","250","250","250","250"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["","","","","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(4) - MCA represents maximum input current.","(4) - MCA represents maximum input current.","(4) - MCA represents maximum input current.","(4) - MCA represents maximum input current."]
["","","","","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA"]