{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EPGA11DAV37","EPGA14DAV37","EPGA16DAV37"]
["Sound pressure level","Heating","","Nom.","dBA","48.0 (2)","49.0 (2)"]
["","Cooling","","Nom.","dBA","55.0 (3)","55.0 (3)"]
["Sound power level","Heating","","Nom.","dBA","64.0 (1)","64.0 (1)"]
["","Cooling","","Nom.","dBA","68.0 (1)","68.0 (1)"]
["Refrigerant","GWP","","","","675.0","675.0"]
["","Charge","","","kg","3.50","3.50"]
["","Type","","","","R-32","R-32"]
["Dimensions","Unit","","Width","mm","1,160","1,160"]
["","","","Depth","mm","380","380"]
["","","","Height","mm","1,440","1,440"]
["Weight","Unit","","","kg","143","143"]
["Operation range","Cooling","","Max.","°CDB","43","43"]
["","","","Min.","°CDB","10","10"]
["","Domestic hot water","","Min.","°CDB","-28","-28"]
["","","","Max.","°CDB","35","35"]
["Piping connections","Level difference","IU - OU","Max.","m","10.0","10.0"]
["Power supply","Phase","","","","1N~","1N~"]
["","Name","","","","V3","V3"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Current","Recommended fuses","","","A","32","32"]
["Notes","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3"]
["","","","","","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT ="]
["Dimensions","Unit","","Height","mm","","","1440"]
["","","","Width","mm","","","1160"]
["","","","Depth","mm","","","380"]
["Weight","Unit","","","kg","","","143"]
["Operation range","Cooling","","Min.","°CDB","","","10"]
["","","","Max.","°CDB","","","43"]
["","Domestic hot water","","Min.","°CDB","","","-28"]
["","","","Max.","°CDB","","","35"]
["Sound power level","Heating","","Nom.","dBA","","","66"]
["","Cooling","","Nom.","dBA","","","68"]
["Sound pressure level","Heating","","Nom.","dBA","","","52.0 (2)"]
["","Cooling","","Nom.","dBA","","","55"]
["Refrigerant","Type","","","","","","R-32"]
["","GWP","","","","","","675"]
["","Charge","","","tCO2Eq","","","2.36"]
["","Charge","","","kg","","","3.5"]
["Piping connections","Level difference","IU - OU","Max.","m","","","10.0"]
["Power supply","Name","","","","","","V3"]
["","Phase","","","","","","1N~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","230"]
["Current","Recommended fuses","","","A","","","32"]