{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","EPRA14DAV37","EPRA16DAV37","EPRA18DAV37"]
["Dimensions","Unit","","Height","mm","1003","1003","1003"]
["","","","Width","mm","1270","1270","1270"]
["","","","Depth","mm","533","533","533"]
["Weight","Unit","","","kg","146","146","146"]
["Operation range","Cooling","","Min.","°CDB","10","10","10"]
["","","","Max.","°CDB","43","43","43"]
["","Domestic hot water","","Min.","°CDB","-28","-28","-28"]
["","","","Max.","°CDB","35","35","35"]
["Sound power level","Heating","","Nom.","dBA","56.0 (1)","56.0","59.0"]
["","Cooling","","Nom.","dBA","65.0 (2)","65.0","65.0"]
["Sound pressure level","Heating","","Nom.","dBA","43.0 (3)","43.0","48.0"]
["","Cooling","","Nom.","dBA","52","52","52"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Charge","","","tCO2Eq","2.84","2.84","2.84"]
["","Charge","","","kg","4.2","4.2","4.2"]
["Piping connections","Level difference","IU - OU","Max.","m","10.0","10.0","10.0"]
["Power supply","Name","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Current","Recommended fuses","","","A","32","32","32"]
["Notes","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3"]
["","","","","","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT ="]
["","","","","","(5) - Percentage of heating capacity at Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(5) - Percentage of heating capacity at Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(5) - Percentage of heating capacity at Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]