{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":8,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERQ-AV1"]
[]
[]
[]
[]
["","","","","","ERQ100A7V1B","ERQ125A7V1B","ERQ140A7V1B"]
["Sound pressure level","Heating","","Nom.","dBA","","53","55"]
["","Cooling","","Nom.","dBA","","51","53"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","8.4","8.4"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","4.0","4.0"]
["","Type","","","","","R-410A","R-410A"]
["Operation range","Cooling","","Max.","°CDB","","46","46"]
["","","","Min.","°CDB","","-5","-5"]
["","Heating","","Max.","°CWB","","15.5","15.5"]
["","","","Min.","°CWB","","-20","-20"]
["Cooling capacity","Nom.","","","kW","","14.0 (1)","15.5 (1)"]
["Piping connections","Liquid","","OD","mm","","9.52","9.52"]
["","","","Type","","","Flare connection","Flare connection"]
["","Gas","","OD","mm","","15.9","19.1"]
["","","","Type","","","Flare connection","Braze connection"]
["","Drain","","OD","mm","","26x3","26x3"]
["","","","Quantity","","","3","3"]
["Power input","Cooling","","Nom.","kW","","3.51 (1)","4.53 (1)"]
["Sound power level","Cooling","","Nom.","dBA","","67","69"]
["COP","","","","","4.56 (2)","4.15 (2)","3.94 (2)"]
["Dimensions","Unit","","Width","mm","","900","900"]
["","","","Depth","mm","","320","320"]
["","","","Height","mm","","1,345","1,345"]
["Weight","Unit","","","kg","","120","120"]
["Fan","Air flow rate","Heating","Nom.","m³/min","","105","105"]
["","","Cooling","Nom.","m³/min","","106","106"]
["EER","","","","","3.99 (1)","3.99 (1)","3.42 (1)"]
["Heating capacity","Nom.","","","kW","","16.0 (2)","18.0 (2)"]
["Power supply","Phase","","","","","1N~","1N~"]
["","Name","","","","","V1","V1"]
["","Frequency","","","Hz","","50","50"]
["","Voltage","","","V","","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal); level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal); level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal); level difference: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","","","(3) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(3) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","","(4) - Sound values are measured in a semi-anechoic room.","(4) - Sound values are measured in a semi-anechoic room."]
["","","","","","","(5) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(5) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA"]
["","","","","","","(9) - Use a circuit breaker instead of a fuse. MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(9) - Use a circuit breaker instead of a fuse. MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","","(10) - MSC means the maximum current during start up of the compressor","(10) - MSC means the maximum current during start up of the compressor"]
["","","","","","","(11) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(11) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","","","(12) - Ssc: Short-circuit power","(12) - Ssc: Short-circuit power"]
["","","","","","","(13) - Contains fluorinated greenhouse gases","(13) - Contains fluorinated greenhouse gases"]
["Cooling capacity","Nom.","","","kW","11.2 (1)"]
["Heating capacity","Nom.","","","kW","12.5 (2)"]
["Power input","Cooling","","Nom.","kW","2.81 (1)"]
["","Heating","","Nom.","kW","2.74 (2)"]
["Dimensions","Unit","","Height","mm","1345"]
["","","","Width","mm","900"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","120"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","106"]
["","","Heating","Nom.","m³/min","102"]
["Operation range","Cooling","","Min.","°CDB","-5"]
["","","","Max.","°CDB","46"]
["","Heating","","Min.","°CWB","-20"]
["","","","Max.","°CWB","15.5"]
["Sound power level","Cooling","","Nom.","dBA","66"]
["Sound pressure level","Cooling","","Nom.","dBA","50"]
["","Heating","","Nom.","dBA","52"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","4"]
["","Charge","","","tCO2Eq","8.4"]
["","GWP","","","","2087.5"]
["Piping connections","Liquid","","Type","","Flare connection"]
["","","","OD","mm","9.52"]
["","Gas","","Type","","Flare connection"]
["","","","OD","mm","15.9"]
["","Drain","","Quantity","","3"]
["","","","OD","mm","26x3"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1N~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]
["Standard Accessories","Connection pipes","","","","","","3"]