{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBH16E6V7 / EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","ETBH16EF6V7 / EPRA14DAV37","ETBH16EF6V7 / EPRA16DAV37","ETBH16EF6V7 / EPRA18DAV37"]
["Heating capacity","Min.","","","kW","3.70","3.96","4.40"]
["","Nom.","","","kW","5.69","9.00","9.00"]
["","Max.","","","kW","10.18","10.91","12.12"]
["Power input","Heating","","Min.","kW","0.88","0.95","1.05"]
["","","","Nom.","kW","1.22","1.80","1.80"]
["","","","Max.","kW","2.09","2.24","2.49"]
["COP","","","","","4.67","5.00","5.00"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.58","3.58","3.58"]
["","","","Seasonal space heating eff. class","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.51","4.51","4.51"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]