{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX12E6V / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETBX12EF6V / EPRA08EAW1","ETBX12EF6V / EPRA10EAW1","ETBX12EF6V / EPRA12EAW1"]
["Indoor unit","","","","","ETBX12EF6V","ETBX12EF6V","ETBX12EF6V"]
["Heating capacity","Min.","","","kW","3.44 (1)","3.44 (1)","3.44 (1)"]
["","Nom.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Max.","","","kW","7.95 (1)","9.25 (1)","9.97 (1)"]
["Cooling capacity","Nom.","","","kW","6.81 (3), 6.47 (4)","7.97 (3), 6.47 (4)","8.62 (3), 6.47 (4)"]
["Power input","Heating","","Min.","kW","0.7 (5)","0.7 (5)","0.7 (5)"]
["","","","Nom.","kW","1.21 (2)","1.21 (2)","1.21 (2)"]
["","","","Max.","kW","1.63 (5)","1.98 (5)","2.21 (5)"]
["","Cooling","","Nom.","kW","2.08 (3), 1.13 (4)","2.57 (3), 1.13 (4)","2.86 (3), 1.13 (4)"]
["COP","","","","","5.1 (2)","5.1 (2)","5.1 (2)"]
["EER","","","","","3.28 (3), 5.75 (4)","3.1 (3), 5.75 (4)","3.01 (3), 5.75 (4)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.59","3.6","3.6"]
["","","","Seasonal space heating eff. class","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.95","4.98","4.98"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]