{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX16E / EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","ETSX16P30EF / EPRA14DAV37","ETSX16P50EF / EPRA14DAV37","ETSX16P30EF / EPRA16DAV37","ETSX16P50EF / EPRA16DAV37","ETSX16P30EF / EPRA18DAV37","ETSX16P50EF / EPRA18DAV37"]
["Heating capacity","Min.","","","kW","37.00 (1)","37.00 (1)","396.00 (1)","396.00 (1)","44.00 (1)","44.00 (1)"]
["","Nom.","","","kW","569 (2)","569 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)"]
["","Max.","","","kW","1,018.00 (1)","1,018.00 (1)","1,091.00 (1)","1,091.00 (1)","1,212.00 (1)","1,212.00 (1)"]
["Cooling capacity","Nom.","","","kW","1,060 (3), 69.0 (4)","1,060 (3), 69.0 (4)","1,150 (3), 788 (4)","1,150 (3), 788 (4)","1,250 (3), 886 (4)","1,250 (3), 886 (4)"]
["Power input","Heating","","Min.","kW","88.00 (5)","88.00 (5)","95.00 (5)","95.00 (5)","105.00 (5)","105.00 (5)"]
["","","","Nom.","kW","122 (2)","122 (2)","18.0 (2)","18.0 (2)","18.0 (2)","18.0 (2)"]
["","","","Max.","kW","209.00 (5)","209.00 (5)","224.00 (5)","224.00 (5)","249.00 (5)","249.00 (5)"]
["","Cooling","","Nom.","kW","255 (3), 256 (4)","255 (3), 256 (4)","28.0 (3), 293 (4)","28.0 (3), 293 (4)","305 (3), 331 (4)","305 (3), 331 (4)"]
["COP","","","","","467.00 (2)","467.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)"]
["EER","","","","","413.00 (3), 27.00 (4)","413.00 (3), 27.00 (4)","411.00 (3), 269.00 (4)","411.00 (3), 269.00 (4)","409.00 (3), 268.00 (4)","409.00 (3), 268.00 (4)"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.62","3.62","3.62","3.62","3.62","3.62"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.57","4.57","4.57","4.57","4.57","4.57"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]