{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":17,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETVH16UE6V7 / EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","ETVH16SU18EA6V7 / EPRA14DAV37","ETVH16SU23EA6V7 / EPRA14DAV37","ETVH16SU18EJ6V7 / EPRA14DAV37","ETVH16SU23EJ6V7 / EPRA14DAV37","ETVH16SU18EA6V7 / EPRA16DAV37","ETVH16SU23EA6V7 / EPRA16DAV37","ETVH16SU18EJ6V7 / EPRA16DAV37","ETVH16SU23EJ6V7 / EPRA16DAV37","ETVH16SU18EA6V7 / EPRA18DAV37","ETVH16SU23EA6V7 / EPRA18DAV37","ETVH16SU18EJ6V7 / EPRA18DAV37","ETVH16SU23EJ6V7 / EPRA18DAV37"]
["Heating capacity","Min.","","","kW","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)"]
["","Nom.","","","kW","5.69 (2)","5.69 (2)","5.69 (2)","5.69 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)"]
["","Max.","","","kW","10.18 (1)","10.18 (1)","10.18 (1)","10.18 (1)","10.91 (1)","10.91 (1)","10.91 (1)","10.91 (1)","12.12 (1)","12.12 (1)","12.12 (1)","12.12 (1)"]
["Power input","Heating","","Min.","kW","0.88 (5)","0.88 (5)","0.88 (5)","0.88 (5)","0.95 (5)","0.95 (5)","0.95 (5)","0.95 (5)","1.05 (5)","1.05 (5)","1.05 (5)","1.05 (5)"]
["","","","Nom.","kW","1.22 (2)","1.22 (2)","1.22 (2)","1.22 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)"]
["","","","Max.","kW","2.09 (5)","2.09 (5)","2.09 (5)","2.09 (5)","2.24 (5)","2.24 (5)","2.24 (5)","2.24 (5)","2.49 (5)","2.49 (5)","2.49 (5)","2.49 (5)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.57 (6)","2.85 (6)","2.57 (6)","2.85 (6)","2.57 (6)","2.85 (6)","2.57 (6)","2.85 (6)","2.57 (6)","2.85 (6)","2.57 (6)","2.85 (6)"]
["Heat up time from 10°C to 50°C","hr","","","","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature"]
["COP","","","","","4.67 (2)","4.67 (2)","4.67 (2)","4.67 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL","L","XL","L","XL","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A","A","A","A","A","A","A","A","A","A","A","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.58","3.58","3.58","3.58","3.58","3.58","3.58","3.58","3.58","3.58","3.58","3.58"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.51","4.51","4.51","4.51","4.51","4.51","4.51","4.51","4.51","4.51","4.51","4.51"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]