{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":17,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETVX16E6V7 / EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","ETVX16S23EJ6V7 / EPRA14DAV37","ETVX16S18EJ6V7 / EPRA14DAV37","ETVX16S23EA6V7 / EPRA14DAV37","ETVX16S18EA6V7 / EPRA14DAV37","ETVX16S18EJ6V7 / EPRA16DAV37","ETVX16S23EJ6V7 / EPRA16DAV37","ETVX16S23EA6V7 / EPRA16DAV37","ETVX16S18EA6V7 / EPRA16DAV37","ETVX16S18EJ6V7 / EPRA18DAV37","ETVX16S23EJ6V7 / EPRA18DAV37","ETVX16S23EA6V7 / EPRA18DAV37","ETVX16S18EA6V7 / EPRA18DAV37"]
["Heating capacity","Min.","","","kW","3.70 (1)","3.70 (1)","","","3.96 (1)","","","","4.40 (1)"]
["","Nom.","","","kW","5.69 (2)","5.69 (2)","","","9.00 (2)","","","","9.00 (2)"]
["","Max.","","","kW","10.18 (1)","10.18 (1)","","","10.91 (1)","","","","12.12 (1)"]
["Cooling capacity","Nom.","","","kW","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","","","11.5 (3), 7.88 (4)","","","","12.5 (3), 8.86 (4)"]
["Power input","Heating","","Min.","kW","0.88 (5)","0.88 (5)","","","0.95 (5)","","","","1.05 (5)"]
["","","","Nom.","kW","1.22 (2)","1.22 (2)","","","1.80 (2)","","","","1.80 (2)"]
["","","","Max.","kW","2.09 (5)","2.09 (5)","","","2.24 (5)","","","","2.49 (5)"]
["","Cooling","","Nom.","kW","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","","","2.80 (3), 2.93 (4)","","","","3.05 (3), 3.31 (4)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.85 (6)","2.57 (6)","","","2.57 (6)","","","","2.57 (6)"]
["Heat up time from 10°C to 50°C","hr","","","","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature"]
["COP","","","","","4.67 (2)","4.67 (2)","4.67","4.67","5.00 (2)","5.00","5.00","5.00","5.00 (2)","5.00","5.00","5.00"]
["EER","","","","","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13, 2.70","4.13, 2.70","4.11 (3), 2.69 (4)","4.11, 2.69","4.11, 2.69","4.11, 2.69","4.09 (3), 2.68 (4)","4.09, 2.68","4.09, 2.68","4.09, 2.68"]
["Domestic hot water heating","General","","Declared load profile","","XL","L","","","L","","","","L"]
["","Average climate","","Water heating energy efficiency class","","A","A","","","A","","","","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.62","3.62","","","3.62","","","","3.62"]
["","","","Seasonal space heating eff. class","","A++","A++","","","A++","","","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.57","4.57","","","4.57","","","","4.57"]
["","","","Seasonal space heating eff. class","","A+++","A+++","","","A+++","","","","A+++"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["Heating capacity","Min.","","","kW","","","3.70","3.70","","3.96","3.96","3.96","","4.40","4.40","4.40"]
["","Nom.","","","kW","","","5.69","5.69","","9.00","9.00","9.00","","9.00","9.00","9.00"]
["","Max.","","","kW","","","10.18","10.18","","10.91","10.91","10.91","","12.12","12.12","12.12"]
["Cooling capacity","Nom.","","","kW","","","10.6, 6.90","10.6, 6.90","","11.5, 7.88","11.5, 7.88","11.5, 7.88","","12.5, 8.86","12.5, 8.86","12.5, 8.86"]
["Power input","Heating","","Min.","kW","","","0.88","0.88","","0.95","0.95","0.95","","1.05","1.05","1.05"]
["","","","Nom.","kW","","","1.22","1.22","","1.80","1.80","1.80","","1.80","1.80","1.80"]
["","","","Max.","kW","","","2.09","2.09","","2.24","2.24","2.24","","2.49","2.49","2.49"]
["","Cooling","","Nom.","kW","","","2.55, 2.56","2.55, 2.56","","2.80, 2.93","2.80, 2.93","2.80, 2.93","","3.05, 3.31","3.05, 3.31","3.05, 3.31"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","","","2.85","2.57","","2.85","2.85","2.57","","2.85","2.85","2.57"]
["Domestic hot water heating","General","","Declared load profile","","","","XL","L","","XL","XL","L","","XL","XL","L"]
["","Average climate","","Water heating energy efficiency class","","","","A","A","","A","A","A","","A","A","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","","3.62","3.62","","3.62","3.62","3.62","","3.62","3.62","3.62"]
["","","","Seasonal space heating eff. class","","","","A++","A++","","A++","A++","A++","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","","4.57","4.57","","4.57","4.57","4.57","","4.57","4.57","4.57"]
["","","","Seasonal space heating eff. class","","","","A+++","A+++","","A+++","A+++","A+++","","A+++","A+++","A+++"]