{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":11,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETVZ16E6V / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETVZ16S23EA6V / EPRA14DAW1","ETVZ16S18EA6V / EPRA14DAW1","ETVZ16S23EA6V / EPRA16DAW1","ETVZ16S18EA6V / EPRA16DAW1","ETVZ16S23EA6V / EPRA18DAW1","ETVZ16S18EA6V / EPRA18DAW1"]
["Domestic hot water heating","General","","Declared load profile","","XL","","XL","","XL"]
["","Average climate","","Water heating energy efficiency class","","A","","A","","A"]
["COP","","","","","4.79 (2)","4.79 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","186","","186","","186"]
["","","","Seasonal space heating eff. class","","A+++","","A+++","","A+++"]
["","","","SCOP","","4.71","","4.71","","4.71"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","","A++","","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","140","","140","","140"]
["","","","SCOP","","3.57","","3.57","","3.57"]
["Heat up time from 10°C to 50°C","hr","","","","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h13min at 7°C ambient temperature","1h02min at 7°C ambient temperature"]
["Heating capacity","Nom.","","","kW","5.90 (2)","","9.00 (2)","","9.00 (2)"]
["","Min.","","","kW","3.70 (1)","","3.96 (1)","","4.40 (1)"]
["","Max.","","","kW","9.75 (1)","","10.44 (1)","","11.60 (1)"]
["Power input","Heating","","Max.","kW","2.17 (5)","","2.32 (5)","","2.58 (5)"]
["","","","Min.","kW","0.84 (5)","","0.90 (5)","","1.00 (5)"]
["","","","Nom.","kW","1.23 (2)","","1.80 (2)","","1.80 (2)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.85 (6)","","2.85 (6)","","2.85 (6)"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["Heating capacity","Min.","","","kW","","3.70 (1)","","3.96 (1)","","4.40 (1)"]
["","Nom.","","","kW","","5.90 (2)","","9.00 (2)","","9.00 (2)"]
["","Max.","","","kW","","9.75 (1)","","10.44 (1)","","11.60 (1)"]
["Power input","Heating","","Min.","kW","","0.84 (5)","","0.90 (5)","","1.00 (5)"]
["","","","Nom.","kW","","1.23 (2)","","1.80 (2)","","1.80 (2)"]
["","","","Max.","kW","","2.17 (5)","","2.32 (5)","","2.58 (5)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","","2.57 (6)","","2.57 (6)","","2.57 (6)"]
["Domestic hot water heating","General","","Declared load profile","","","L","","L","","L"]
["","Average climate","","Water heating energy efficiency class","","","A","","A","","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","3.57","","3.57","","3.57"]
["","","","Seasonal space heating eff. class","","","A++","","A++","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","4.71","","4.71","","4.71"]
["","","","Seasonal space heating eff. class","","","A+++","","A+++","","A+++"]
["Energy Efficiency Range","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]