{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EVLQ05CAV3","EVLQ08CAV3"]
["Dimensions","Unit","","Height","mm","735","735"]
["","","","Width","mm","832","832"]
["","","","Depth","mm","307","307"]
["Weight","Unit","","","kg","54","56"]
["Fan","Air flow rate","Heating","High","m³/min","45.0","47.0"]
["","","Cooling","High","m³/min","525","525"]
["Operation range","Heating","","Min.","°CWB","-25","-25"]
["","","","Max.","°CWB","25","25"]
["Sound power level","Heating","","Nom.","dBA","61","62"]
["Sound pressure level","Heating","","Nom.","dBA","48 (1)","49 (1)"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","GWP","","","","2088","2088"]
["","Charge","","","tCO2Eq","3.0","3.3"]
["","Charge","","","kg","1.5","1.6"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","159","159"]
["","Drain","","OD","mm","1x ø15 + 1x ø20","1x ø15 + 1x ø20"]
["","Level difference","IU - OU","Max.","m","20.0","20.0"]
["Power supply","Name","","","","V3","V3"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Current","Recommended fuses","","","A","16","20"]
["Notes","","","","","(1) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(1) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(2) - Standard on/off compressor starting current >> max. running current","(2) - Standard on/off compressor starting current >> max. running current"]
["","","","","","(3) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(3) - Daikin Altherma inverter controlled compressor starting current always <= max. running current"]