{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWSAH-UD9W"]
[]
[]
[]
[]
["","","","","","EWSAH06UDA9W"]
["Refrigerant","Charge","","","TCO2Eq","1.15"]
["","GWP","","","","675.0"]
["","Charge","","","kg","1.70"]
["","Type","","","","R-32"]
["Operation range","Installation space","","Min.","°C","5"]
["","","","Max.","°C","35"]
["","Heating","Water side","Max.","°C","65"]
["","","","Min.","°C","5"]
["","Domestic hot water","Water side","Max.","°C","60"]
["","","","Min.","°C","25"]
["Dimensions","Unit","","Width","mm","597"]
["","","","Depth","mm","666"]
["","","","Height","mm","1,891"]
["Casing","Material","","","","Precoated sheet metal"]
["","Colour","","","","White + Black"]
["Tank","Water volume","","","l","180"]
["","Corrosion protection","","","","Pickling"]
["","Insulation","","Heat loss","kWh/24h","1.4"]
["Weight","Unit","","","kg","222"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","252"]
["","","","Seasonal space heating eff. class","","A+++"]
["","","","SCOP","","6.49 (1)"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A+++"]
["","","","ηs (Seasonal space heating efficiency)","%","158"]
["","","","SCOP","","4.15 (1)"]
["Power supply","Phase","","","","1~/3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230/400"]
["Current","Recommended fuses","","","A","16/32"]
["Notes","","","","","(1) - According to EN14825 and EN14511:2018"]