{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWSAX-UD9W"]
[]
[]
[]
[]
["","","","","","EWSAX06UDA9W"]
["Casing","Colour","","","","White + Black"]
["","Material","","","","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1891"]
["","","","Width","mm","597"]
["","","","Depth","mm","666"]
["Weight","Unit","","","kg","222"]
["Tank","Water volume","","","l","180"]
["","Insulation","","Heat loss","kWh/24h","1.4"]
["","Corrosion protection","","","","Pickling"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","tCO2Eq","1.15"]
["","Charge","","","kg","1.70"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","4.24"]
["","","","Seasonal space heating eff. class","","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","6.68"]
["","","","Seasonal space heating eff. class","","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Power supply","Phase","","","","1~/3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230/400"]
["Current","Recommended fuses","","","A","16/32"]
["Notes","","","","","(1) - According to EN14825 and EN14511:2018"]