{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWWT-Q-XRA"]
[]
[]
[]
[]
["","","","","","EWWT100Q-XRA1","EWWT125Q-XRA1","EWWT160Q-XRA1"]
["Cooling capacity","Nom.","","","kW","96.36","124.4","166"]
["Capacity control","Method","","","","Step","Step","Step"]
["","Minimum capacity","","","%","50","50","50"]
["Power input","Cooling","","Nom.","kW","20.99","27.95","34.44"]
["EER","","","","","4.59","4.45","4.82"]
["IPLV","","","","","7.15","7.12","7.41"]
["SEER","","","","","6.4","6.54","6.49"]
["Dimensions","Unit","","Depth","mm","1300","1300","1300"]
["","","","Height","mm","1000","1000","1000"]
["","","","Width","mm","1200","1200","1200"]
["Weight","Operation weight","","","kg","490","542","612"]
["","Unit","","","kg","470","520","582"]
["Casing","Colour","","","","Ivory white","Ivory white","Ivory white"]
["","Material","","","","Galvanized and painted steel sheet","Galvanized and painted steel sheet","Galvanized and painted steel sheet"]
["Water heat exchanger - evaporator","Water pressure drop","Cooling","Nom.","kPa","19.35","19.98","22.15"]
["Compressor","Quantity","","","","2","2","2"]
["","Type","","","","Scroll","Scroll","Scroll"]
["Operation range","Water side","Evaporator","Min.","°CDB","-15","-15","-15"]
["","","","Max.","°CDB","30","30","30"]
["Sound power level","Cooling","","Nom.","dBA","74.99","78.19","79.99"]
["Sound pressure level","Cooling","","Nom.","dBA","59.36","62.56","64.36"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","6","7.1","9.1"]
["","Circuits","","Quantity","","1","1","1"]
["Piping connections","Evaporator water inlet/outlet (OD)","","","","3\"","3\"","3\""]
["Power supply","Phase","","","","3","3","3"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["","Voltage range","","Min.","%","-10","-10","-10"]
["","","","Max.","%","10","10","10"]
["Unit","Starting current","","Max","A","221","345","363"]
["","Running current","Cooling","Nom.","A","36.6","44.2","52.6"]
["","","","Max","A","62","80","97"]
["","Max unit current for wires sizing","","","A","68","88","107"]