{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":9,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-R"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35R5V1B","FCAG50BVEB / RXM50R2V1B","FCAG50BVEB / RXM50R5V1B","FCAG60BVEB / RXM60R5V1B","FCAG60BVEB / RXM60R2V1B"]
["Cooling capacity","Nom.","","kW","","5.00","5.00","5.70","5.70"]
["Heating capacity","Nom.","","kW","","6.00","6.00","7.00","7.00"]
["Nominal efficiency","Annual energy consumption","","kWh","","698","698","858","858"]
["","COP","","","","3.70","3.70","3.38","3.38"]
["","EER","","","","3.58","3.58","3.31","3.31"]
["","Energy labeling Directive","Cooling","","","A","A","A","A"]
["","","Heating","","","A","A","C","C"]
["Space cooling","Annual energy consumption","","kWh/a","","268","268","312","312"]
["","Energy efficiency class","","","","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","5.00","5.00","5.70","5.70"]
["","SEER","","","","6.54","6.54","6.40","6.40"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","1,418","1,418","1,569","1,569"]
["","Capacity","Pdesign","kW","","4.36","4.36","4.71","4.71"]
["","Energy efficiency class","","","","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","","3.86","3.86","4.12","4.12"]
["","SCOP/A","","","","4.30","4.30","4.20","4.20"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","3.50"]
["Heating capacity","Nom.","","kW","4.20"]
["Nominal efficiency","EER","","","3.72"]
["","COP","","","3.77"]
["","Annual energy consumption","","kWh","470"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","3.50"]
["","SEER","","","6.35"]
["","Annual energy consumption","","kWh/a","193"]
["Space heating (Average climate)","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","3.32"]
["","SCOP/A","","","4.90"]
["","Pdh Heating capacity at -10°","","kW","2.60"]
["","Annual energy consumption","","kWh/a","948"]
["Energy Efficiency Range","","","","A+++ ~ D"]