{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","","","","","","6.80","6.80","13.40"]
["Space cooling","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Annual energy consumption","","kWh/a","","","","","","","345","345","1,191"]
["","Capacity","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Energy efficiency class","","","","","","","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Energy efficiency class","","","","","","","","","A+","A+"]
["","Annual energy consumption","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Nominal efficiency","EER","","","","","","","","","4.09","4.09","3.18"]
["Notes","","","","","","","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Nominal efficiency","Annual energy consumption","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Energy labeling Directive","Cooling","","","","","","","","","A"]
["","","Heating","","","","","","","","","A"]
["Heating capacity","Nom.","","kW","","","","","","","","7.50","15.50"]
["Notes","","","","","","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Space cooling","ηs,c","","%","","","","","","","","","266.88"]
["Space heating (Average climate)","ηs,h","","%","","","","","","","","","172.10"]