{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F / 3MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F2V1B / FDXM25F2V1B / 3MXM40M2V1B","FDXM25F2V1B / FDXM35F2V1B / 3MXM40M2V1B","FDXM35F2V1B / FDXM35F2V1B / 3MXM40M2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00"]
["Space cooling","SEER","","","6.73","6.64","6.59"]
["","Annual energy consumption","","kWh/a","208","211","213"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00"]
["","Energy efficiency class","","","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.80","4.80","5.00"]
["","SCOP/A","","","3.80","3.82","3.94"]
["","Energy efficiency class","","","A","A","A"]
["","Annual energy consumption","","kWh/a","1,768","1,756","1,773"]
["Nominal efficiency","EER","","","4.02","3.96","4.00"]
["","Annual energy consumption","","kWh","498","505","500"]
["","COP","","","3.61","3.65","3.95"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","4.60","4.60","4.60"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]