{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":12,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / RZASG71M2V1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZASG100M7V1B","FFA50A2VEB9 / FFA50A2VEB9 / RZASG100M7V1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZASG125M7V1B","FFA60A2VEB9 / FFA60A2VEB9 / RZASG125M7V1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZASG125M7V1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZASG140M7V1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZASG140M7V1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","","","12.1 (1)","11.4 (1)","","13.4 (1)","13.4 (1)"]
["Space cooling","SEER","","","6.12","","","6.90","5.30","","8.49","6.99"]
["","Annual energy consumption","","kWh/a","389","","","1,052","753","","947","1,150"]
["","Capacity","Pdesign","kW","6.80","","","12.1","11.4","","13.4","13.4"]
["","Energy efficiency class","","","A++","","","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","","","6.00","6.00","","7.80","7.00"]
["","SCOP/A","","","3.84","","","4.34","3.80","","4.79","4.31"]
["","Energy efficiency class","","","A","","","","A"]
["","Annual energy consumption","","kWh/a","1,641","","","1,936","2,211","","2,281","2,273"]
["Heating capacity","Nom.","","kW","7.50 (2)","","","13.5 (2)","13.5 (2)","","15.5 (2)","15.5 (2)"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","9.50","9.50","","","12.1"]
["Heating capacity","Nom.","","kW","","10.8","10.8","","","13.5"]
["Space cooling","Energy efficiency class","","","","A++","A"]
["","Capacity","Pdesign","kW","","9.50","9.50","","","12.1"]
["","SEER","","","","6.24","5.49","","","6.29"]
["","Annual energy consumption","","kWh/a","","533","606","","","1154"]
["Space heating (Average climate)","Energy efficiency class","","","","A","A"]
["","Capacity","Pdesign","kW","","6.00","6.00","","","6.00"]
["","SCOP/A","","","","3.82","3.90","","","4.39"]
["","Annual energy consumption","","kWh/a","","2199","2154","","","1914"]