{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZAG-B"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RZAG35B5V1B","FHA35AVEB98 / RZAG35B5V1B","FHA50AVEB98 / RZAG50B5V1B","FHA71AVEB98 / RZAG60B5V1B","FHA60AVEB98 / RZAG60B5V1B"]
["Cooling capacity","Min.","","kW","1.7","1.7","1.7","1.9","1.9"]
["","Nom.","","kW","3.5","3.5","5","6","6"]
["","Max.","","kW","4.5","4.5","6","6.8","6.8"]
["Heating capacity","Min.","","kW","1.4","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","4","4","5.8","7","7"]
["","Max.","","kW","5.5","5.5","6.5","7.5","7.5"]
["Nominal efficiency","EER","","","5.05","4.6","4.1","4.35","3.9"]
["","COP","","","4.18","4.1","3.71","3.52","3.4"]
["","Annual energy consumption","","kWh","347","380","610","690","769"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","B","C"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","3.5","3.5","5","6","6"]
["","SEER","","","6.65","6.4","6.8","6.81","6.6"]
["","Annual energy consumption","","kWh/a","184","191","257","308","318"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","3.1","3.1","4","4.6","4.6"]
["","SCOP/A","","","4.18","4.1","4.3","4.35","4.2"]
["","Pdh Heating capacity at -10°","","kW","2.77","2.75","3.46","3.96","3.93"]
["","Annual energy consumption","","kWh/a","1038","1058","1302","1480","1633"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]