{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / RXF-A"]
[]
[]
[]
[]
["","","","","FTXF71F2V1B / RXF71A2V1B","FTXF71F2V1B / RXF71A5V1B"]
["Outdoor unit","","","","RXF71A2V1B","RXF71A5V1B"]
["Cooling capacity","Min.","","kW","2.3","2.3"]
["","Nom.","","kW","7.1","7.1"]
["","Max.","","kW","7.3","7.3"]
["Heating capacity","Min.","","kW","2.3","2.3"]
["","Nom.","","kW","8.2","8.2"]
["","Max.","","kW","9","9"]
["Nominal efficiency","EER","","","2.56","2.56"]
["","COP","","","3.15","3.15"]
["","Annual energy consumption","","kWh","1387","1387"]
["","Energy labeling Directive","Cooling","","E","E"]
["","","Heating","","D","D"]
["Space cooling","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","7.1","7.1"]
["","SEER","","","5.15","5.15"]
["","Annual energy consumption","","kWh/a","483","483"]
["Space heating (Average climate)","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","6.2","6.2"]
["","SCOP/A","","","3.81","3.81"]
["","Pdh Heating capacity at -10°","","kW","5.02","5.02"]
["","Annual energy consumption","","kWh/a","2278","2278"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]