{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":12,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F"]
[]
[]
[]
[]
["","","","","","FTXF20F5V1B","FTXF25F5V1B (Archived)","FTXF35F5V1B (Archived)","FTXF42F5V1B (Archived)","FTXF50F5V1B (Archived)","FTXF60F2V1B (Archived)","FTXF71F2V1B (Archived)"]
["Power input","Cooling","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.032","0.032"]
["","Heating","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.035","0.035"]
["Casing","Colour","","","","White","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","286","286","286","286","286","295","295"]
["","","","Width","mm","770","770","770","770","770","990","990"]
["","","","Depth","mm","225","225","225","225","225","263","263"]
["Weight","Unit","","","kg","8","8","8.5","9","9","13.5","13.5"]
["Fan","Air flow rate","Cooling","High","m³/min","9.8","10","11.5","12.6","12.6","17.3","17.3"]
["","","","Medium","m³/min","8","8","8","9","9","14.8","14.8"]
["","","","Low","m³/min","6","6.2","6.4","6.9","7.2","12.2","12.2"]
["","","","Silent operation","m³/min","4.3","4.3","4.4","4.9","6.4","10.7","10.7"]
["","","Heating","High","m³/min","10.4","10.4","11.9","12.8","12.8","17.9","17.9"]
["","","","Medium","m³/min","8.3","8.4","8.6","8.8","9.6","15.8","15.8"]
["","","","Low","m³/min","6.2","6.4","6.5","6.7","7.2","12.8","12.8"]
["","","","Silent operation","m³/min","5.3","5.3","5.3","5.2","6.4","11.3","11.3"]
["Sound power level","Cooling","","","dBA","53","54","54","59","59","60","62"]
["","Heating","","","dBA","55","55","56","59","59","62","62"]
["Sound pressure level","Cooling","","High","dBA","39","40","43","45","45","45","46"]
["","","","Medium","dBA","33","33","34","36","39","41","42"]
["","","","Low","dBA","25","26","27","30","34","36","37"]
["","","","Silent operation","dBA","20","20","20","22","31","33","34"]
["","Heating","","High","dBA","39","40","40","44","44","44","45"]
["","","","Medium","dBA","34","34","35","34","38","40","41"]
["","","","Low","dBA","28","28","29","28","33","35","36"]
["","","","Silent operation","dBA","21","21","21","22","30","32","33"]
["Piping connections","Liquid","","OD","mm","6","6","6","6","6","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Drain","","","","18","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC470A1","ARC470A1"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["Power supply","Name","","","","","","","","","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-440","220-440","220-440","220-440","220-440","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]