{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ25A2V1BS / RXJ25M5V1B9"]
["Outdoor unit","","","","RXJ25M5V1B9"]
["Cooling capacity","Nom.","","kW","2.40"]
["Heating capacity","Nom.","","kW","3.20"]
["Nominal efficiency","EER","","","4.73"]
["","COP","","","4.57"]
["","Annual energy consumption","","kWh","254"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A+++"]
["","Capacity","Pdesign","kW","2.40"]
["","SEER","","","8.64"]
["","Annual energy consumption","","kWh/a","97"]
["Space heating (Average climate)","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","2.70"]
["","SCOP/A","","","4.60"]
["","Pdh Heating capacity at -10°","","kW","2.18"]
["","Annual energy consumption","","kWh/a","822"]
["Energy Efficiency Range","","","","A+++ ~ D"]