{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":23,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A / 3MXM-A8"]
[]
[]
[]
[]
["","","","","FTXM20A2V1B / FTXM20A2V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM20A2V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM20A5V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM20A5V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM20A5V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM20A5V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A2V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM20A5V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM25A2V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM25A2V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM25A2V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B8","FTXM25A5V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B8","FTXM25A5V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B8"]
["Cooling capacity","Nom.","","kW","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20"]
["Heating capacity","Nom.","","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80"]
["Nominal efficiency","EER","","","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76"]
["","COP","","","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88"]
["","Annual energy consumption","","kWh","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546"]
["","Energy labeling Directive","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Capacity","Pdesign","kW","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20","5.20"]
["","SEER","","","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51"]
["","Annual energy consumption","","kWh/a","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214"]
["Space heating (Average climate)","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Capacity","Pdesign","kW","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["","SCOP/A","","","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10"]
["","Pdh Heating capacity at -10°","","kW","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10","4.10"]
["","Annual energy consumption","","kWh/a","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373","1,373"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]