{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B (Archived)","FTXM25K3V1B (Archived)","FTXM35K3V1B (Archived)","FTXM42K3V1B (Archived)","FTXM50K3V1B (Archived)"]
["Sound pressure level","Heating","High","dBA","40","41","45","45","47"]
["","","Silent operation","dBA","19","19","19","22","24"]
["","","Low","dBA","27","27","29","33","34"]
["","Cooling","Silent operation","dBA","19","19","19","21","23"]
["","","Low","dBA","24","25","29","33","34"]
["","","High","dBA","40","41","45","45","46"]
["","","Nom.","dBA","34","34","39","39","40"]
["","Cooling","Nom.","dBA","32","33","37","39","40"]
["Standard Accessories","Operation manual","","","1","1","1","1","1"]
["","Installation manual","","","1","1","1","1","1"]
["","Infrared remote control","","","1","1","1","1","1"]
["","Batteries","","","2","2","2","2","2"]
["","Mounting plate","","","1","1","1","1","1"]
["","Indoor unit fixing screws","","","2","2","2","2","2"]
["","Titanium apatite photocatalytic air purification filter","","","2","2","2","2","2"]
["","Remote control holder","","","1","1","1","1","1"]
["Control systems","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","12.7","12.7"]
["","Drain","","","18","18","18","18","18"]
["Sound power level","Cooling","","dBA","56","57","59","59","60"]
["","Heating","","dBA","56","57","59","59","60"]
["Dimensions","Unit","Width","mm","780","780","900","900","900"]
["","","Depth","mm","215","215","215","215","215"]
["","","Height","mm","289","289","298","298","298"]
["Casing","Colour","","","White","White","White","White","White"]
["Weight","Unit","","kg","8","8","11","11","11"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]