{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":18,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 3MXM-A8"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / FTXM20R5V1B / 3MXM40A2V1B8","FTXM20R2V1B / FTXM20R2V1B / 3MXM40A2V1B8","FTXM25R5V1B / FTXM25R5V1B / 3MXM52A2V1B8","FTXM25R2V1B / FTXM25R2V1B / 3MXM52A2V1B8","FTXM35R2V1B / FTXM35R2V1B / 3MXM68A2V1B8","FTXM35R5V1B / FTXM35R5V1B / 3MXM68A2V1B8","FTXM20R5V1B / FTXM20R5V1B / FTXM25R2V1B / 3MXM68A2V1B8","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / 3MXM68A2V1B8","FTXM20R5V1B / FTXM25R5V1B / FTXM25R5V1B / 3MXM68A2V1B8","FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 3MXM68A2V1B8","FTXM20R5V1B / FTXM50R2V1B / 3MXM68A2V1B8","FTXM20R2V1B / FTXM50R2V1B / 3MXM68A2V1B8","FTXM25R5V1B / FTXM42R5V1B / 3MXM68A2V1B8","FTXM25R2V1B / FTXM42R2V1B / 3MXM68A2V1B8"]
["Cooling capacity","Nom.","","kW","4.00","4.00","5.00","5.00","6.8","6.8","6.5","6.5","6.8","6.8","6.8","6.8","6.7","6.7"]
["Heating capacity","Nom.","","kW","4.60","4.60","6.80","6.80","8.60","8.60","8.20","8.20","8.60","8.60","8.60","8.60","8.30","8.30"]
["Nominal efficiency","EER","","","4.76","4.76","4.85","4.85","3.94","3.94","4.01","4.01","3.85","3.85","3.59","3.59","3.74","3.74"]
["","COP","","","4.73","4.73","4.45","4.45","3.81","3.81","4.49","4.49","4.38","4.38","3.82","3.82","3.95","3.95"]
["","Annual energy consumption","","kWh","420","420","515","515","863","863","810","810","883","883","947","947","896","896"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++","A+++","A+++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","4.00","4.00","5.00","5.00","6.80","6.80","6.50","6.50","6.80","6.80","6.80","6.80","6.70","6.70"]
["","SEER","","","8.53","8.53","8.59","8.59","6.97","6.97","7.76","7.76","7.71","7.71","6.75","6.75","6.94","6.94"]
["","Annual energy consumption","","kWh/a","164","164","204","204","342","342","294","294","309","309","352","352","338","338"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A","A","A","A"]
["","Capacity","Pdesign","kW","4.80","4.80","4.80","4.80","4.80","4.80","5.30","5.30","5.30","5.30","4.50","4.50","4.30","4.30"]
["","SCOP/A","","","4.25","4.25","4.38","4.38","4.00","4.00","4.09","4.09","4.10","4.10","3.90","3.90","3.86","3.86"]
["","Pdh Heating capacity at -10°","","kW","3.60","3.60","3.90","3.90","3.73","3.73","4.21","4.21","4.21","4.21","3.55","3.55","3.41","3.41"]
["","Annual energy consumption","","kWh/a","1,582","1,582","1,533","1,533","1,680","1,680","1,814","1,814","1,807","1,807","1,612","1,612","1,559","1,559"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]