{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M / RXP-N"]
[]
[]
[]
[]
["","","","","FTXP50M2V1B / RXP50N5V1B","FTXP60M2V1B / RXP60N5V1B","FTXP71M2V1B / RXP71N5V1B"]
["Cooling capacity","Min.","","kW","1.7","1.7","2.3"]
["","Nom.","","kW","5.0","6.0","7.1"]
["","Max.","","kW","6.0","7.0","7.3"]
["Heating capacity","Min.","","kW","1.7","1.7","2.3"]
["","Nom.","","kW","6.0","7.0","8.2"]
["","Max.","","kW","7.7","8.0","9.0"]
["Nominal efficiency","Annual energy consumption","","kWh","693","912","1,345"]
["","COP","","","3.80","3.63","3.19"]
["","EER","","","3.61","3.29","2.64"]
["","Energy labeling Directive","Cooling","","A","A","D"]
["","","Heating","","A","A","D"]
["Space cooling","Annual energy consumption","","kWh/a","240","308","401"]
["","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","5.0","6.0","7.1"]
["","SEER","","","7.30","6.82","6.20"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","1,463","1,638","2,166"]
["","Capacity","Pdesign","kW","4.60","4.80","6.20"]
["","Energy efficiency class","","","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","3.15","3.29","4.24"]
["","SCOP/A","","","4.40","4.10","4.01"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]