{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Power input","Cooling","","Nom.","kW","0.02","0.02","0.03"]
["","Heating","","Nom.","kW","0.02","0.03","0.03"]
["Casing","Colour","","","","White","White","White"]
["Dimensions","Unit","","Height","mm","600","600","600"]
["","","","Width","mm","750","750","750"]
["","","","Depth","mm","238","238","238"]
["Weight","Unit","","","kg","17","17","17"]
["Fan","Air flow rate","Cooling","High","m³/min","8.7","9.2","11.6"]
["","","","Medium","m³/min","7","7","9"]
["","","","Low","m³/min","4.9","4.9","6.6"]
["","","","Silent operation","m³/min","4.1","4.1","5.4"]
["","","Heating","High","m³/min","9.2","9.8","12.8"]
["","","","Medium","m³/min","7.2","7.2","10"]
["","","","Low","m³/min","5.6","5.6","8.4"]
["","","","Silent operation","m³/min","4.1","4.1","5.9"]
["Sound power level","Cooling","","","dBA","52","53","61"]
["","Heating","","","dBA","52","53","62"]
["Sound pressure level","Cooling","","High","dBA","38","39","44"]
["","","","Medium","dBA","32","32","38"]
["","","","Low","dBA","25","25","31"]
["","","","Silent operation","dBA","20","20","27"]
["","Heating","","High","dBA","38","39","46"]
["","","","Medium","dBA","32","32","40"]
["","","","Low","dBA","25","25","35"]
["","","","Silent operation","dBA","19","19","29"]
["Refrigerant","GWP","","","","675","675","675"]
["Piping connections","Liquid","","OD","mm","6.4","6.4","6.4"]
["","Gas","","OD","mm","9.5","9.5","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Energy Efficiency Range","","","","","A+++ ~ D"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]