{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXNQ-A"]
[]
[]
[]
[]
["","","","","","FXNQ20A2VEB","FXNQ25A2VEB","FXNQ32A2VEB","FXNQ40A2VEB","FXNQ50A2VEB","FXNQ63A2VEB"]
["Cooling capacity","Total capacity","","At high fan speed","kW","2.20","2.80","3.60","4.50","5.60","7.10"]
["Heating capacity","Total capacity","","At high fan speed","kW","2.50","3.20","4.00","5.00","6.30","8.00"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.071","0.071","0.071","0.078","0.099","0.110"]
["","Heating","","At high fan speed","kW","0.068","0.068","0.068","0.075","0.096","0.107"]
["Dimensions","Unit","","Height","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["","","","Width","mm","790","790","790","990","990","1,190"]
["","","","Depth","mm","200","200","200","200","200","200"]
["Weight","Unit","","","kg","23.5","23.5","23.5","27.5","27.5","32.0"]
["Casing","Colour","","","","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted"]
["","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","8.0","8.0","8.0","10.5","12.5","16.5"]
["","","","At low fan speed","m³/min","6.4","6.4","6.4","8.5","10.0","13.0"]
["","External static pressure - 50Hz","","High","Pa","41.0","41.0","42.0","52.0","59.0","55.0"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Sound power level","Cooling","","At high fan speed","dBA","51","51","51","52","53","54"]
["Sound pressure level","Cooling","","At high fan speed","dBA","30.0","30.0","30.0","32.0","33.0","35.0"]
["","","","At medium fan speed","dBA","28.5","28.5","28.5","30.0","31.0","33.0"]
["","","","At low fan speed","dBA","27.0","27.0","27.0","28.0","29.0","32.0"]
["","Heating","","At high fan speed","dBA","30.0","30.0","30.0","32.0","33.0","35.0"]
["","","","At medium fan speed","dBA","28.5","28.5","28.5","30.0","31.0","33.0"]
["","","","At low fan speed","dBA","27.0","27.0","27.0","28.0","29.0","32.0"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","","","OD","mm","6.35","6.35","6.35","6.35","6.35","9.52"]
["","Gas","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","","","OD","mm","12.7","12.7","12.7","12.7","12.7","15.9"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Air filter","Type","","","","Resin net","Resin net","Resin net","Resin net","Resin net","Resin net"]
["Power supply","Name","","","","VE","VE","VE","VE","VE","VE"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","16","16","16","16","16","16"]
["Notes","","","","","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs"]
["","","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(3) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(4) - Select wire size based on the value of MCA","(4) - Select wire size based on the value of MCA","(4) - Select wire size based on the value of MCA","(4) - Select wire size based on the value of MCA","(4) - Select wire size based on the value of MCA","(4) - Select wire size based on the value of MCA"]
["","","","","","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(6) - Use a circuit breaker instead of a fuse.","(6) - Use a circuit breaker instead of a fuse.","(6) - Use a circuit breaker instead of a fuse.","(6) - Use a circuit breaker instead of a fuse.","(6) - Use a circuit breaker instead of a fuse.","(6) - Use a circuit breaker instead of a fuse."]
["","","","","","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere.","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere.","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere.","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere.","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere.","(7) - MCA/MFA; MCA= 1,25 x FLA; MFA=< 4 x FLA; The next lower standard fuse rating is minimum 16 ampere."]
["","","","","","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases"]
["","","","","","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A"]