{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HCU-PXB1"]
[]
[]
[]
[]
["","","","","","HCU2040PXB1","HCU4070PXB1"]
["Refrigerating capacity","Low temperature","","Nom.","kW","3.03","6.56"]
["Compressor","Number of revolutions","","","rpm","4,800","3,600"]
["Weight","Unit","","","kg","161","300"]
["Fan motor","Output","","","W","115","230"]
["","Drive","","","","EC","EC"]
["Heat exchanger","Type","","","","Standard Cu-Al.","Standard Cu-Al."]
["Power input","Low temperature","","Nom.","kW","3.79","7.05"]
["COP","Low temperature","","Nom.","","0.80","0.93"]
["Dimensions","Unit","","Width","mm","574","773"]
["","","","Depth","mm","1,452","1,684"]
["","","","Height","mm","799","1,438"]
["Fan motor 2","Output","","","W","115","230"]
["Casing","Colour","","","","Light grey RAL 7035","Light grey RAL 7035"]
["Fan","Type","","","","Axial","Axial"]
["","Quantity","","","","1","2"]
["","Air flow rate","Cooling","Nom.","m³/min","63","126"]
["Current","Nominal running current (RLA) - 50Hz","Compressor 1","Cooling","A","15.00","13.70"]