{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HXY-A8"]
[]
[]
[]
[]
["","","","","HXY080A8V1BF","HXY125A8V1BF","HXY080A8V1B (Archived)","HXY125A8V1B (Archived)"]
["Sound pressure level","Nom.","","dBA","31 (4)","31 (4)","31 (4)","31 (4)"]
["Refrigerant","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Type","","","R-410A","R-410A","R-410A","R-410A"]
["Dimensions","Unit","Width","mm","480","480","480","480"]
["","","Depth","mm","344","344","344","344"]
["","","Height","mm","890","890","890","890"]
["Casing","Material","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","White","White","White","White"]
["Weight","Unit","","kg","44.0","44.0","44.0","44.0"]
["PED","Category","","","Art3§3, Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Art3§3, Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Art3§3, Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Art3§3, Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["Wiring connections","For connection with user interface","Quantity","","2","2","2","2"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Current","Recommended fuses","","A","6~16","6~16","6~16","6~16"]
["Notes","","","","(1) - Tamb 35°C - LWE 18°C (DT=5°C)","(1) - Tamb 35°C - LWE 18°C (DT=5°C)","(1) - Tamb 35°C - LWE 18°C (DT=5°C)","(1) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(3) - Flow switch setting","(3) - Flow switch setting","(3) - Flow switch setting","(3) - Flow switch setting"]
["","","","","(4) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(4) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(4) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(4) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases"]