{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":8,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LREN-A"]
[]
[]
[]
[]
["","","","","","LREN8A7Y1B","LREN10A7Y1B","LREN12A7Y1B"]
["Refrigerating capacity","Low temperature","","Nom.","kW","11.2 (3)","13.5 (3)","15.5 (3)"]
["","Medium temperature","","Nom.","kW","19.8 (4)","23.1 (4)","26.3 (4)"]
["Power input","Low temperature","","Nom.","kW","11.6 (3)","14.1 (3)","16.9 (3)"]
["","Medium temperature","","Nom.","kW","10.7 (4)","13.2 (4)","15.5 (4)"]
["COP","Low temperature","","Nom.","","0.97 (3)","0.96 (3)","0.92 (3)"]
["","Medium temperature","","Nom.","","1.86 (4)","1.75 (4)","1.69 (4)"]
["Casing","Colour","","","","Ivory white","Ivory white","Ivory white"]
["Dimensions","Unit","","Height","mm","1,680","1,680","1,680"]
["","","","Width","mm","1,930","1,930","1,930"]
["","","","Depth","mm","765","765","765"]
["Weight","Unit","","","kg","547","547","547"]
["Fan","Type","","","","Propeller fan","Propeller fan","Propeller fan"]
["","Quantity","","","","3","3","3"]
["","Air flow rate","Cooling","Nom.","m³/min","285 (6)","285 (6)","315 (6)"]
["Fan motor","Output","","","W","750","750","750"]
["","Drive","","","","Direct drive","Direct drive","Direct drive"]
["Heat exchanger","Type","","","","Cross fin coil (waffle louver fins and Hi-X tubes)","Cross fin coil (waffle louver fins and Hi-X tubes)","Cross fin coil (waffle louver fins and Hi-X tubes)"]
["Refrigerant","Type","","","","R744 (CO2)","R744 (CO2)","R744 (CO2)"]
["","GWP","","","","1.0","1.0","1.0"]
["","Charge","","","kg","0.00 (7)","0.00 (7)","0.00 (7)"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Declaration of conformity","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Auxiliary piping set","","","","1","1","1"]
["","Safety valve pipe","","","","1","1","1"]
["","Safety valve","","","","1","1","1"]
["","Stop valve body insulation","","","","1","1","1"]
["","Stop valve cap insulation","","","","1","1","1"]
["Power supply","Phase","","","","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415"]
["Notes","","","","","(1) - Minimum load of each individual refrigeration indoor unit: 3 KW (for Medium Temperature Operation)","(1) - Minimum load of each individual refrigeration indoor unit: 3 KW (for Medium Temperature Operation)","(1) - Minimum load of each individual refrigeration indoor unit: 3 KW (for Medium Temperature Operation)"]
["","","","","","(2) - Minimum load of each individual refrigeration indoor unit: 2 KW (for Low Temperature Operation).","(2) - Minimum load of each individual refrigeration indoor unit: 2 KW (for Low Temperature Operation).","(2) - Minimum load of each individual refrigeration indoor unit: 2 KW (for Low Temperature Operation)."]
["","","","","","(3) - Rated conditions: saturation temperature equivalent to suction pressure: -35°C (LT),outdoor temp. 32°C, Suction SH 10K","(3) - Rated conditions: saturation temperature equivalent to suction pressure: -35°C (LT),outdoor temp. 32°C, Suction SH 10K","(3) - Rated conditions: saturation temperature equivalent to suction pressure: -35°C (LT),outdoor temp. 32°C, Suction SH 10K"]
["","","","","","(4) - Rated conditions: saturation temperature equivalent to suction pressure: -10°C (MT), outdoor temp. 32°C, Suction SH 10K","(4) - Rated conditions: saturation temperature equivalent to suction pressure: -10°C (MT), outdoor temp. 32°C, Suction SH 10K","(4) - Rated conditions: saturation temperature equivalent to suction pressure: -10°C (MT), outdoor temp. 32°C, Suction SH 10K"]
["","","","","","(5) - Every compressor equipped with 1 accumulator of 0,909 liters.","(5) - Every compressor equipped with 1 accumulator of 0,909 liters.","(5) - Every compressor equipped with 1 accumulator of 0,909 liters."]
["","","","","","(6) - Outdoor Unit Total Airflow","(6) - Outdoor Unit Total Airflow","(6) - Outdoor Unit Total Airflow"]
["","","","","","(7) - The unit is not pre-charged. A minimal rest charge is present related to factory quality inspection","(7) - The unit is not pre-charged. A minimal rest charge is present related to factory quality inspection","(7) - The unit is not pre-charged. A minimal rest charge is present related to factory quality inspection"]
["","","","","","(8) - Compressor 1","(8) - Compressor 1","(8) - Compressor 1"]
["","","","","","(9) - Compressor 2","(9) - Compressor 2","(9) - Compressor 2"]
["","","","","","(10) - Compressor 3","(10) - Compressor 3","(10) - Compressor 3"]
["","","","","","(11) - Factory charge of unit","(11) - Factory charge of unit","(11) - Factory charge of unit"]
["","","","","","(12) - Sound pressure data: measured at 1m in front of unit, at 1.5m height. Nominal operation condition – Medium evaporation temperature (MT)","(12) - Sound pressure data: measured at 1m in front of unit, at 1.5m height. Nominal operation condition – Medium evaporation temperature (MT)","(12) - Sound pressure data: measured at 1m in front of unit, at 1.5m height. Nominal operation condition – Medium evaporation temperature (MT)"]
["","","","","","(13) - For MT (Medium Temperature) Operation","(13) - For MT (Medium Temperature) Operation","(13) - For MT (Medium Temperature) Operation"]
["","","","","","(14) - For LT (Low Temperature) Operation","(14) - For LT (Low Temperature) Operation","(14) - For LT (Low Temperature) Operation"]
["","","","","","(15) - Compressor 1: 2Y190CPCY1P#C; Compressor 2: 2Y190CPCY1P#C; Compressor 3: 2Y190CPDY1P#C","(15) - Compressor 1: 2Y190CPCY1P#C; Compressor 2: 2Y190CPCY1P#C; Compressor 3: 2Y190CPDY1P#C","(15) - Compressor 1: 2Y190CPCY1P#C; Compressor 2: 2Y190CPCY1P#C; Compressor 3: 2Y190CPDY1P#C"]
["","","","","","(16) - Only K65 (or equivalent) with D.P. 90 bar is allowed to use for refrigeration piping.","(16) - Only K65 (or equivalent) with D.P. 90 bar is allowed to use for refrigeration piping.","(16) - Only K65 (or equivalent) with D.P. 90 bar is allowed to use for refrigeration piping."]
["","","","","","(17) - For all the LRNUN5A7Y1 specifications, please refer to the related MDM drawing","(17) - For all the LRNUN5A7Y1 specifications, please refer to the related MDM drawing","(17) - For all the LRNUN5A7Y1 specifications, please refer to the related MDM drawing"]