{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Standard Accessories","Declaration of conformity","","","","1"]
["Weight","Unit","","","kg","173"]
["Refrigerant","GWP","","","","1.0"]
["","Type 2","","","","R-744"]
["","Charge","","","kg","3.20"]
["Fan motor","Output","","","W","350"]
["Heat exchanger","Type","","","","Cross fin coil"]
["Dimensions","Unit","","Width","mm","635"]
["","","","Depth","mm","765"]
["","","","Height","mm","1,680"]
["Casing","Colour","","","","Ivory white"]
["Fan","Type","","","","Propeller fan"]
["","Quantity","","","","1"]
["","Air flow rate","Cooling","Nom.","m³/min","102"]
["Power supply","Phase","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Notes","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Compressor 1"]
["","","","","","(3) - Compressor 2"]
["","","","","","(4) - Compressor 3"]
["","","","","","(5) - Factory charge of unit"]
["","","","","","(6) - Only K65 with D.P. 120 bar is allowed to use for AC piping connections."]
["","","","","","(7) - The safety valve pressure is indicated as gauge pressure."]
["","","","","","(8) - Only K65 with D.P. 90 bar is allowed to use for refrigeration piping."]