{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80ZB"]
[]
[]
[]
[]
["","","","","","MC80ZBFVM"]
["Type","","","","","Air Purifier"]
["Application","","","","","Floor standing type"]
["Casing","Colour","","","","Front: White, Top/Side: Dark Grey"]
["Dimensions","Unit","","Height","mm","630"]
["","","","Width","mm","315"]
["","","","Depth","mm","315"]
["Weight","Unit","","","kg","9.8"]
["Applicable room area","m²","","","","62 (1), 124 (2)"]
["CADR","m³/h","","","","480"]
["Air purifying operation","Power input","","Turbo","kW","0.08"]
["","","","M","kW","0.016"]
["","","","L","kW","0.011"]
["","","","Silent","kW","0.009"]
["Sound pressure level","Air purifying operation","","Turbo","dBA","55"]
["","","","Medium","dBA","34"]
["","","","Low","dBA","25"]
["","","","Silent","dBA","19"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","480"]
["","","","Medium","m³/h","210"]
["","","","Low","m³/h","132"]
["","","","Silent","m³/h","84"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Twin streamer + Deodorizing catalyst"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Power cord","m","","","","2"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Notes","","","","","(1) - The coverage area is appropriate for operating the unit of maximum fan speed(HH). Coverage area indicates the space where a certain amount of dust particles can be removed in 30 minutes."]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]