{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70ZBFW"]
[]
[]
[]
[]
["","","","","","MCK70ZBFVMW"]
["Type","","","","","Humidifying air purifier"]
["Application","","","","","Floor standing type"]
["Casing","Colour","","","","White (9.9YR/9.4/0.2)"]
["Dimensions","Unit","","Height","mm","760"]
["","","","Width","mm","315"]
["","","","Depth","mm","315"]
["Weight","Unit","","","kg","12.5"]
["Applicable room area","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Air purifying operation","Power input","","Turbo","kW","0.082"]
["","","","M","kW","0.020"]
["","","","L","kW","0.011"]
["","","","Silent","kW","0.010"]
["Humidifying operation","Power input","","Turbo","kW","0.084"]
["","","","M","kW","0.023"]
["","","","L","kW","0.012"]
["","","","Silent","kW","0.010"]
["","Water tank capacity","","","l","3.4"]
["Sound pressure level","Air purifying operation","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Low","dBA","27"]
["","","","Silent","dBA","18"]
["","Humidifying operation","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Low","dBA","27"]
["","","","Silent","dBA","18"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Low","m³/h","132"]
["","","","Silent","m³/h","84"]
["","","Humidifying operation","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Low","m³/h","132"]
["","","","Silent","m³/h","84"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Standard Accessories","Electrostatic HEPA filter","","","","1"]
["","Humidifying filter","","","","2"]
["","Deodorising filter","","","","1"]
["","Installation and operation manual","","","","1"]
["","Caster","","","","4"]
["Power cord","m","","","","2"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Notes","","","","","(1) - The coverage area is appropriate for operating the unit of maximum fan speed(HH). Coverage area indicates the space where a certain amount of dust particles can be removed in 30 minutes."]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]
["","","","","","(3) - Converted to CADR standards from test values in accordance with JEM1467."]
["","","","","","(4) - Humidification amount changes in accordance with indoor and outdoor temperature and humidity. Measurement condition: 20°C in temperature, 30% in humidity."]
["","","","","","(5) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]
["","","","","","(6) - Electrostatic HEPA filter and humidifying filters are attached in the unit."]
["","","","","","(7) - Requirements according to JEM1467."]
["","","","","","(8) - \"HI\" is displayed when the PM2.5 concentration exceeds 99µg/m3."]