{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-GVB"]
[]
[]
[]
[]
["","","","","","RX60G4V1B","RX71GV1B8"]
["Sound pressure level","Heating","","High","dBA","49","52"]
["","","","Low","dBA","46","49"]
["","Cooling","","Low","dBA","46","49"]
["","","","High","dBA","49","52"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug (only heat pump models)","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","3.1","4.8"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","1.5","2.3"]
["","Type","","","","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","680","730"]
["","","Heating","Super low","rpm","680","730"]
["Piping connections","Level difference","IU - OU","Max.","m","20","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","825","900"]
["","","","Depth","mm","300","320"]
["","","","Height","mm","735","770"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","47","71"]
["Fan","Air flow rate","Heating","Super low","cfm","1,497","1,624"]
["","","Cooling","Super low","cfm","1,497","1,624"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 230V","(3) - 230V"]
["","","","","","(4) - 240V","(4) - 240V"]
["","","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Drain socket","","","","","1"]